{"text_format":"1","workbook":"xlsx","n_sheets":2,"sheets":["Teste de Bombeamento","Interpretação Gráfica"],"not_rendered":{"charts":2,"images":1,"macros":1,"external_links":0,"defined_names":1,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Teste de Bombeamento","index":0,"n_rows":34,"n_cols":11,"rows_kept":34,"cut":false,"hidden":false,"merged":[[4,1,4,3],[6,1,6,3],[11,1,12,1],[33,1,36,10],[11,9,12,9],[11,8,12,8],[11,3,12,3],[11,5,12,5],[10,6,10,10],[10,1,10,5],[11,6,12,6],[7,4,7,6],[8,7,8,10],[7,7,7,10],[9,1,9,3],[9,4,9,10],[5,4,5,6],[11,7,12,7],[11,10,12,10],[11,4,12,4],[1,1,1,10],[2,1,2,10],[6,4,6,6],[4,7,4,10],[8,1,8,6],[5,7,5,10],[5,1,5,3],[7,1,7,3],[6,7,6,10],[3,1,3,10],[4,4,4,6],[11,2,12,2]]}
[]
[null,"SECRETARIA DE ESTADO DO DESENVOLVIMENTO AMBIENTAL – SEDAM\nCOORDENADORIA DE RECURSOS HÍDRICOS – COREH\nAv. Farquar, nº 2986 – Complexo Rio Madeira – Edifício Rio Cautário – Térreo\nBairro Pedrinhas – Porto Velho-RO. CEP 76.801-470\n Fone/Fax: +55(69) 3212-9617/98482-8512\nEmail: sedamrecursoshidricos@gmail.com / coreh@sedam.ro.gov.br"]
[null,"FICHA PARA TESTE DE BOMBEAMENTO E RECUPERAÇÃO"]
[null,"Município/UF: "]
[null,"Poço nº: ",null,null,"Prof. do Poço (m): ",null,null,"Nível Estático (m): "]
[null,"Elevação (m): ",null,null,"Diâmetro (Pol.):",null,null,"Nível Dinâmico (m): "]
[null,"Executor:",null,null,"Boca do Poço (m): ",null,null,"Vazão Média (m³/h): "]
[null,"Data de Início: ",null,null,"Data de Término: ",null,null,"Tempo Bomb. (h): "]
[null,"Coordenada Geográfica: SIRGAS 2000 ",null,null,null,null,null,"Profund. Crivo (m): "]
[null,"Cota Topográfica (m):",null,null,"Método Utilizado no Teste de Bombeamento:"]
[null,"Bombeamento",null,null,null,null,"Recuperação"]
[null,"HORA","t (min)","N.D. (m)","Sw (m)","Q (m³/h)","HORA","t' (min)","N.D. (m)","Sw (m)","tb/t' +1 (min)"]
[]
[null,"08:01:00",1,5.5,{"$f":"D14-5","v":0.5},2,"20:31:00",1,15,{"$f":"I14-5","v":10},{"$f":"360/H14+1","v":361}]
[null,"08:02:00",2,6,{"$f":"D15-5","v":1},2,"20:32:00",2,14.5,{"$f":"I15-5","v":9.5},{"$f":"360/H15+1","v":181}]
[null,"08:03:00",3,6.5,1.5,2,"20:33:00",3,14,9,121]
[null,"08:04:00",4,7,2,2,"20:34:00",4,13.5,8.5,91]
[null,"08:05:00",5,7.5,2.5,2,"20:35:00",5,13,8,73]
[null,"08:06:00",6,8,3,2,"20:36:00",6,12.5,7.5,61]
[null,"08:08:00",8,8.5,3.5,2,"20:38:00",8,12,7,46]
[null,"08:10:00",10,9,4,2,"20:40:00",10,11.5,6.5,37]
[null,"08:12:00",12,9.5,4.5,2,"20:42:00",12,11,6,31]
[null,"08:15:00",15,10,5,2,"20:45:00",15,10.5,5.5,25]
[null,"08:20:00",20,10.5,5.5,2,"20:50:00",20,10,5,19]
[null,"08:25:00",25,11,6,2,"20:55:00",25,9.5,4.5,15.4]
[null,"08:30:00",30,11.5,6.5,2,"21:00:00",30,9,4,13]
[null,"08:40:00",40,12,7,2,"21:10:00",40,8.5,3.5,10]
[null,"08:50:00",50,12.5,7.5,2,"21:20:00",50,8,3,8.1999999999999993]
[null,"09:00:00",60,13,8,2,"21:30:00",60,7.5,2.5,7]
[null,"09:10:00",70,13.5,8.5,2,"21:40:00",70,7,2,6.1428571428571432]
[null,"09:20:00",80,14,9,2,"21:50:00",80,6.5,1.5,5.5]
[null,"09:40:00",100,14.5,9.5,2,"22:10:00",100,6,1,4.5999999999999996]
[null,"10:00:00",120,15,10,2,"22:20:00",120,5.5,0.5,4]
[null,"Observações:"]

{"sheet":"Interpretação Gráfica","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[]}